# Source code for tecplot.data.extract

    import ctypes

    from ..tecutil import _tecutil
    from ..constant import *
    from ..exception import *
    from .. import layout, macro, tecutil, version
    from ..tecutil import sv

    @tecutil.lock()
    def extract_blanked_zones(*zones, **kwargs):
        """Extract subsets of `Zones`_ based on blanking conditions of the plot.

        Parameters:
            *zones (`Zones`_, required): Set of source zones to extract.

        Keyword Arguments:
            plot (`Cartesian3DFieldPlot` or other data-backed plot type, optional):
                The plot that defines the blanking conditions. By default, the
                active plot will be used.

        Returns:
            `Zones`_: A `list` of the extracted zones.

        A new zone will be created for each zone specified unless blanking dictates
        that all cells and points in the entire zone are blanked. The following
        example extracts all zones in the dataset:

        .. code-block:: python

            import os

            import tecplot as tp
            from tecplot.constant import *

            examples_dir = tp.session.tecplot_examples_directory()
            datafile = os.path.join(examples_dir, 'SimpleData', 'VortexShedding.plt')

            dataset = tp.data.load_tecplot(datafile)

            plot = tp.active_frame().plot()
            plot.show_contour = True

            xax = plot.axes.x_axis
            xax.min = -0.005
            xax.max = 0.015
            yax = plot.axes.y_axis
            yax.min = -0.01
            yax.max = 0.002

            # Setup value blanking
            vblank = plot.value_blanking
            constraint = vblank.constraint(0)
            constraint.variable_index = 1
            constraint.comparison_operator = RelOp.GreaterThan
            constraint.active = True
            vblank.active = True

            # Use list comprehension to get all zones assocaitated with
            # a specific strand, in this case strand 1
            in_zns = [zn for zn in dataset.zones() if zn.strand == 1]

            # Extract all zones assocaitated with strand 1
            ext_zns = tp.data.extract.extract_blanked_zones(in_zns)

            # Place all extracted zones into the same strand
            for zn in ext_zns:
                zn.strand = 2

            # Turn off plotting for the original zone and turn on plotting
            # of the extracted zones.
            plot.fieldmap(0).show = False
            plot.fieldmap(1).show = True

            tp.export.save_time_animation_mpeg4('extract_blanked_zones.mp4',
                                                width=400, end_time=0.0004,
                                                supersample=3)

        .. raw:: html

            <video controls>
                <source src="../_static/videos/extract_blanked_zones.m4v" type="video/mp4">
                I'm sorry; your browser doesn't support HTML5 MPEG4/H.264 video.
            </video>

        .. versionadded:: 2020.1
            Extracting blanked zones requires Tecplot 360 2020 R1 or later.
        """
        if __debug__:
            if version.sdk_version_info < (2020,):
                msg = 'Extracting blanked zones not supported.'
                raise TecplotOutOfDateEngineError((2020,), msg)

        if not zones:
            msg = 'extract_blanked_zones(*zones) requires at least one zone'
            raise TecplotLogicError(msg)
        plot = kwargs.get('plot', None)
        if not plot:
            plot = layout.active_frame().plot()
        dataset = plot.frame.dataset
        num_zones = dataset.num_zones
        with plot.activated():
            zones = tecutil.flatten_args(*zones)
            zone_indices = (getattr(z, 'index', z) for z in zones)
            cmd = 'Zones = [{}]'.format(','.join(str(z + 1) for z in zone_indices))
            macro.execute_extended_command('ExtractBlankedZones', cmd)
        return [dataset.zone(i) for i in range(num_zones, dataset.num_zones)]

    @tecutil.lock()
    def extract_line(points, num_points=None, frame=None, dataset=None):
        """Create new zone from a line in the dataset.

        Parameters:
            points (``2D numeric array``): The points defining the line in two or
                three dimensions. This array must be of the shape *(N, D)* where
                *N* is the number points and *D* is the number of dimensions. That
                is, it must take the form ``[(x0, y0, z0), (x1, y1, z1) ...]``.
                Points that do not lie within the dataset volume will be removed
                from the resulting zone.
            num_points (`int`, optional): The number of points to evenly
                distribute along the polyline. (default: length of *points* or *N*)
            frame (`Frame`, optional): A `Frame` that holds the `Dataset` to
                operate on which must match *dataset* if given. (default: currently
                active `Frame`)
            dataset (`Dataset`, optional): The `Dataset` to operate on which must
                be attached to *frame* if given. (default: currently active
                `Dataset`)

        Returns:
            A 1D `OrderedZone` representing a line through the data. Points outside
            of the dataset will be removed from the extracted zone resulting in
            fewer points than input.

        .. warning::

            Line extraction is only available when the plot type is set to
            `Cartesian2D` or `Cartesian3D`::

                >>> from tecplot.constant import PlotType
                >>> frame.plot_type = PlotType.Cartesian3D

        This example shows how to extract a zone along a line, overlaying the
        result in a new frame:

        .. code-block:: python
            :emphasize-lines: 26

            import numpy as np
            from os import path

            import tecplot as tp
            from tecplot.constant import *

            examples_dir = tp.session.tecplot_examples_directory()
            datafile = path.join(examples_dir, 'SimpleData', 'VortexShedding.plt')
            dataset = tp.data.load_tecplot(datafile)

            frame = tp.active_frame()
            frame.activate()
            plot = frame.plot()
            plot.contour(0).variable = dataset.variable("P(N/M2)")
            plot.show_contour = True
            plot.contour(0).levels.reset(num_levels=11)
            plot.contour(0).colormap_name = 'Sequential - Yellow/Green/Blue'

            plot.axes.y_axis.min = -0.01
            plot.axes.y_axis.max = 0.01
            plot.axes.x_axis.min = -0.005
            plot.axes.x_axis.max = 0.015

            xx = np.linspace(0, 0.01, 100)
            yy = np.zeros(100)
            line = tp.data.extract.extract_line(zip(xx, yy))

            plot.show_mesh = True
            plot.fieldmap(0).mesh.show = False

            frame = tp.active_page().add_frame()
            frame.position = (3.0, 0.5)
            frame.height = 2
            frame.width = 4
            plot = tp.active_frame().plot(PlotType.XYLine)
            plot.activate()

            plot.delete_linemaps()
            lmap = plot.add_linemap('data', line, x=dataset.variable('P(N/M2)'),
                                    y=dataset.variable('T(K)'))
            lmap.line.line_thickness = 2.0
            plot.axes.x_axis(0).title.font.size = 10
            plot.axes.y_axis(0).title.font.size = 10
            plot.axes.viewport.left = 20
            plot.axes.viewport.bottom = 20
            plot.view.fit()

            tp.export.save_png("extract_line.png", region=ExportRegion.AllFrames,
                               width=600, supersample=3)

        .. figure:: /_static/images/extract_line.png
            :width: 300px
            :figwidth: 300px
        """
        if dataset is None:
            if frame is None:
                frame = layout.active_frame()
            dataset = frame.dataset
        elif frame is None:
            frame = dataset.frame

        if __debug__:
            if frame.plot_type not in [PlotType.Cartesian2D, PlotType.Cartesian3D]:
                msg = 'must be in a cartesian plot type to extract a line'
                raise TecplotLogicError(msg)
            if dataset != frame.dataset:
                msg = 'dataset is not attached to given frame'
                raise TecplotLogicError(msg)

        new_zone_index = dataset.num_zones

        try:
            _ = points[0]
        except TypeError:
            points = list(points)

        ndim = len(points[0])
        if num_points is None:
            num_points = len(points)

        n = len(points)
        xx = (ctypes.c_double * n)(*(float(p[0]) for p in points))
        yy = (ctypes.c_double * n)(*(float(p[1]) for p in points))
        zz = (ctypes.c_double * n)(*([0.]*len(xx)
                                     if ndim < 3
                                     else (float(p[2]) for p in points)))

        extract_through_volume = ndim == 3
        only_points_on_line = num_points == len(points)
        include_distance = False
        to_file = False
        filename = None

        try:
            if not _tecutil.ExtractFromPolyline(xx, yy, zz, len(xx),
                                                extract_through_volume,
                                                only_points_on_line,
                                                include_distance, num_points,
                                                to_file, filename):
                raise TecplotSystemError()
        except TecplotLogicError as e:
            # If some of the points are outside of the data, the zone
            # is still extracted and this exception is not technically
            # an error. A different message is generated if all of the
            # points are outside of the data which is re-raised.
            if 'Probe Position is outside of the data' not in str(e):
                raise

        return dataset.zone(new_zone_index)

    @tecutil.lock()
    def extract_slice(origin=(0, 0, 0), normal=(0, 0, 1), source=None,
                      mode=ExtractMode.SingleZone, copy_cell_centers=None,
                      assign_strand_ids=None,
                      transient_mode=TransientOperationMode.SingleSolutionTime,
                      frame=None, dataset=None, **kw):
        """Create new zone from a plane in the dataset.

        Parameters:
            origin (array of three `floats <float>`): Point in space,
                :math:`(x, y, z)`, that lies on the slice plane.
            normal (array of three `floats <float>`): Vector direction,
                :math:`(x, y, z)`, indicating the normal of the slice plane.
            source (`SliceSource`): Source zone types to consider when extracting
                the slice. Possible values: `SliceSource.LinearZones`,
                `SliceSource.SurfaceZones`, `SliceSource.SurfacesOfVolumeZones`,
                `SliceSource.VolumeZones` (default).
            mode (`ExtractMode`): Controls how many zones are created. Possible
                values are: `ExtractMode.SingleZone` (default),
                `ExtractMode.OneZonePerConnectedRegion` and
                `ExtractMode.OneZonePerSourceZone`.
            copy_cell_centers (`bool`): If `True`, cell-center
                values will be copied when possible to the extracted slice plane.
                Cell-centers are copied when a variable is cell-centered for all
                the source zones through which the slice passes. Otherwise,
                extracted planes use node-centered data, which is calculated by
                interpolation. (default: `False`)
            assign_strand_ids (`bool`): Automatically assign strand IDs
                to the data extracted from transient sources. This is only
                available if *multiple_zones* is `False`. (default: `True`)
            transient_mode (`TransientOperationMode`): Determines which solution
                times are used to extract slices when transient data is available
                in the dataset. Possible values are
                `TransientOperationMode.SingleSolutionTime` (default) or
                `TransientOperationMode.AllSolutionTimes`.
            frame (`Frame`, optional): A `Frame` that holds the `Dataset` to
                operate on which must match *dataset* if given. (default: currently
                active `Frame`)
            dataset (`Dataset`, optional): The `Dataset` to operate on which must
                be attached to *frame* if given. (default: currently active
                `Dataset`)

        Returns:
            One or a `list` of `Zones <data_access>` representing a planar slice.

        .. warning::

            Slicing is only available when the plot type is set to 3D::

                >>> from tecplot.constant import PlotType
                >>> frame.plot_type = PlotType.Cartesian3D

        .. note::

            The extracted zone is returned if **mode** is `ExtractMode.SingleZone`
            and **transient_mode** is `TransientOperationMode.SingleSolutionTime`,
            otherwise a `generator <https://docs.python.org/3/reference/expressions.html#generator-expressions>`_
            of the extracted zones.

        .. seealso:: `tecplot.plot.SliceGroup.extract()`

        This example shows extracting a slice zone from the surface a wing:

        .. code-block:: python
            :emphasize-lines: 16-20

            import os
            import tecplot as tp
            from tecplot.constant import PlotType, SliceSource

            examples_dir = tp.session.tecplot_examples_directory()
            datafile = os.path.join(examples_dir, 'OneraM6wing',
                                    'OneraM6_SU2_RANS.plt')
            dataset = tp.data.load_tecplot(datafile)

            frame = tp.active_frame()
            frame.plot_type = PlotType.Cartesian3D

            # set active plot to 3D and extract
            # an arbitrary slice from the surface
            # data on the wing
            extracted_slice = tp.data.extract.extract_slice(
                origin=(0, 0.25, 0),
                normal=(0, 1, 0),
                source=SliceSource.SurfaceZones,
                dataset=dataset)

            # switch plot type in current frame, clear plot
            plot = frame.plot(PlotType.XYLine)
            plot.activate()
            plot.delete_linemaps()

            # create line plot from extracted zone data
            cp_linemap = plot.add_linemap(
                name='Quarter-chord C_p',
                zone=extracted_slice,
                x=dataset.variable('x'),
                y=dataset.variable('Pressure_Coefficient'))

            # set style of linemap plot and
            # update axes limits to show data
            cp_linemap.line.color = tp.constant.Color.Blue
            cp_linemap.line.line_thickness = 0.8
            cp_linemap.y_axis.reverse = True
            plot.view.fit()

            # export image of pressure coefficient as a function of x
            tp.export.save_png('wing_slice_pressure_coeff.png', 600, supersample=3)

        .. figure:: /_static/images/wing_slice_pressure_coeff.png
            :width: 300px
            :figwidth: 300px
        """
        if 'multiple_zones' in kw:
            tecutil.api_changed('''\
                "multiple_zones" has been removed, please use "mode" instead.''',
                '0.13', '2018 R2')

        if dataset is None:
            if frame is None:
                frame = layout.active_frame()
            dataset = frame.dataset
        elif frame is None:
            frame = dataset.frame

        mode = ExtractMode(mode)
        transient_mode = TransientOperationMode(transient_mode)

        if __debug__:
            if frame.dataset != dataset:
                raise TecplotLogicError('Dataset is not attached to frame.')
            if frame.plot_type is not PlotType.Cartesian3D:
                msg = 'Plot Type must be Cartesian3D to create a slice.'
                raise TecplotLogicError(msg)
            if mode != ExtractMode.SingleZone:
                if version.sdk_version_info < (2017, 3):
                    msg = '"mode" parameter not supported.'
                    raise TecplotOutOfDateEngineError((2017, 3), msg)
            if transient_mode != TransientOperationMode.SingleSolutionTime:
                if version.sdk_version_info < (2019, 1):
                    msg = 'Slice over all solution times not supported'
                    raise TecplotOutOfDateEngineError((2019, 1), msg)

        with frame.activated():
            nzones = dataset.num_zones
            with tecutil.ArgList() as arglist:
                arglist[sv.ORIGINX] = float(origin[0])
                arglist[sv.ORIGINY] = float(origin[1])
                arglist[sv.ORIGINZ] = float(origin[2])
                arglist[sv.NORMALX] = float(normal[0])
                arglist[sv.NORMALY] = float(normal[1])
                arglist[sv.NORMALZ] = float(normal[2])
                if source is not None:
                    arglist[sv.SLICESOURCE] = SliceSource(source)
                if mode != ExtractMode.SingleZone:
                    arglist[sv.EXTRACTMODE] = mode
                arglist[sv.COPYCELLCENTEREDVALUES] = copy_cell_centers
                if assign_strand_ids is not None:
                    arglist[sv.AUTOSTRANDTRANSIENTDATA] = bool(assign_strand_ids)
                if transient_mode != TransientOperationMode.SingleSolutionTime:
                    arglist[sv.TRANSIENTOPERATIONMODE] = transient_mode
                if not _tecutil.CreateSliceZoneFromPlneX(arglist):
                    raise TecplotSystemError()
                if dataset.num_zones == nzones:
                    raise TecplotLogicError('No zones found when extracting slice')

            if (
                mode == ExtractMode.SingleZone and
                transient_mode == TransientOperationMode.SingleSolutionTime
            ):
                return dataset.zone(nzones)
            else:
                return (dataset.zone(i) for i in range(nzones, dataset.num_zones))

    @tecutil.lock()
    def extract_zones_from_connected_regions(zones):
        with tecutil.IndexSet(zones) as zone_set:
            if not _tecutil.ExtractZonesFromConnectedRegions(zone_set):
                raise TecplotSystemError()

    @tecutil.lock()
    def triangulate(*zones, **kwargs):
        """Create a new zone by forming triangles from points in 2D zones.

        Arguments:
            *zones (`Zones`_): Set of 2-dimensional source zones to triangulate.

        Keyword Arguments:
            boundary_zones (`list` of :math:`I`-Ordered `Zones`_, optional): Set
                of :math:`I`-ordered zones that define the boundaries across which
                no triangles can be created. (default: `None`)
            include_boundary_points (`bool`, optional): If `True`, boundary points
                will be used to create triangles. (default: `False`)
            keep_factor (`float` in the range [0.0, 0.5], optional): The smaller
                the number, the more likely it will be that highly obtuse triangles
                will be created opening toward the outside of the triangulated
                zone.
            plot (`Cartesian2DFieldPlot`, optional): The plot defining the
                :math:`(x, y)` variables in the dataset. If not set, the active
                plot will be used which must be of type `Cartesian2DFieldPlot`.

        Returns:
            `ClassicFEZone`: The resulting triangulated zone.

        The active plot or the plot specified must be of type
        `Cartesian2DFieldPlot` and the boundary zones, if supplied, may only be
        :math:`I`-ordered zones. This example creates a new zone by triangulating
        data points from two other `Zones`_::

            >>> zone0 = dataset.zone('Zone 0')
            >>> zone1 = dataset.zone('Zone 1')
            >>> new_zone = tp.data.extract.triangulate(zone0, zone1)
        """
        boundary_zones = kwargs.get('boundary_zones', None)
        include_boundary_points = bool(kwargs.get('include_boundary_points', False))
        keep_factor = float(kwargs.get('keep_factor', 0.25))
        plot = kwargs.get('plot', None)
        if not plot:
            plot = layout.active_frame().plot()

        with plot.activated():
            zones = tecutil.flatten_args(*zones)
            dataset = zones[0].dataset
            num_zones = dataset.num_zones
            with tecutil.optional(tecutil.IndexSet, zones) as zones:
                with tecutil.optional(tecutil.IndexSet, boundary_zones) as bzones:
                    res = _tecutil.Triangulate(zones, bool(bzones), bzones,
                                               include_boundary_points, keep_factor)
                    success, num_coincident_points = res
                    if not success:
                        raise TecplotSystemError()
                    return dataset.zone(num_zones)